|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_\_\_\_\_9/29/23\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**    **Inspector (Print Name):\_\_\_\_\_\_\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Nathaniel Wixon Middle School - 901 Route 134, South Dennis, Massachusetts** | | | | | |
| **Location** | **ACBM**  **Description** | **Estimated**  **Quantity** | | **VERTEX**  **April 2013**  **Condition** | **September**  **2023**  **Updated**  **Condition** |
| ***Upper Level-Original Section*** | | | | | |
| Front Entrance | 2' x 4' Ceiling Tile (Fissure) | 1200 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Cloak Room (Room F) | 12" x 12" Brown Spec Floor Tile | 300 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 300 | ft2 | G | G |
| Room E (Police and Supply Room) | 12" x 12" Gray Spec Floor Tile | 418 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 386 | ft2 | 32 ft2 D | MD 8ft2 |
| 266/267/268 Corridor | 2' x 4' Ceiling Tile (Fissure) | 1400 | ft2 | MD | MD |
| Red Duct Mastic (Above Ceiling)1 | 60 | lf | G | G |
| Room 268 (Social Worker Office) | 12" x 12" Brown Spec Floor Tile (Under Carpet) | 400 | ft2 | C | C |
| Contaminated Carpet | 400 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 368 | ft2 | G | G |
| Room 267 | 12" x 12" Brown Spec Floor Tile | 900 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 368 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 266 | 12" x 12" Brown Spec Floor Tile | 900 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 368 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 224/Server Room | 12" x 12" Brown Spec Floor Tile | 340 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 340 | ft2 | G | 2ft2D |
| Room H (Reception) | 2' x 4' Ceiling Tile (Fissure) | 354 | ft2 | G | G |
| Main Office Closet | 12" x 12" Brown Spec Floor Tile | 354 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 354 | ft2 | 4 ft2 D | G |
| Room G | 12" x 12" Brown Spec Floor Tile (Under Carpet) | 310 | ft2 | C | C |
| Contaminated Carpet | 310 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 310 | ft2 | G | G |
| Room I (Principal) | 2' x 4' Ceiling Tile (Fissure) | 280 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Principal Bath | 12" x 12" Brown Spec Floor Tile | 340 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 340 | ft2 | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_\_\_9/29/23\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**    **Inspector (Print Name):\_\_\_\_\_\_\_\_\_\_\_\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Nathaniel Wixon Middle School - 901 Route 134, South Dennis, Massachusetts** | | | | | |
| **Location** | **ACBM**  **Description** | **Estimated**  **Quantity** | | **VERTEX**  **April 2013**  **Condition** | **September**  **2023**  **Updated**  **Condition** |
| ***Upper Level-Original Section (Continued)*** | | | | | |
| Room I-J Hall and Closet | 12" x 12" Brown Spec Floor Tile | 48 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 48 | ft2 | G | G |
| Room J (Dean Office) and Closet | 2' x 4' Ceiling Tile (Fissure) | 280 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room M/K  (Guidance Office) | 2' x 4' Ceiling Tile (Fissure) | 672 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Clinic (Nurse Office) | 12" x 12" Brown Spec Floor Tile | 636 | ft2 | G | G |
| 12" x 12" Gray Spec Floor Tile | 264 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 900 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Copy Room  (in Room 273) | 2' x 4' Ceiling Tile (Fissure) | 144 | ft2 | G | G |
| Room 273 | 2' x 4' Ceiling Tile (Fissure) | 960 | ft2 | 8 ft2 D | G |
| Interior Window Glazing | SU |  | P | P |
| 12" x 12" Tan Floor Tile |  |  | NF\* | NF\* |
| Room 274 | 2' x 4' Ceiling Tile (Fissure) | 960 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| 12" x 12" Tan Floor Tile |  |  | NF\* | NF\* |
| Room 275 | 2' x 4' Ceiling Tile (Fissure) | 880 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| 12" x 12" Tan Floor Tile |  |  | NF\* | NF\* |
| Room 276 | 2' x 4' Ceiling Tile (Fissure) | 640 | ft2 | 32 ft2 D | 32 ft2 D |
| Interior Window Glazing | SU |  | P | P |
| 12" x 12" Tan Floor Tile |  |  | NF\* | NF\* |
| Main Office Corridor (Reception-Nurse) | 2' x 4' Ceiling Tile (Fissure) | 1000 | ft2 | 8 ft2 D | G |
| Red Duct Mastic (Above Ceiling)1 | 70 | lf | G | G |
| 277-279 Corridor | 2' x 4' Ceiling Tile (Fissure) | 1440 | ft2 | MD | 40 ft2 D |
| Interior Window Glazing | SU |  | P | P |
| Room 277 | 12" x 12" Gray Spec Floor Tile | 1320 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 1320 | ft2 | 24 ft2 D | G |
| Interior Window Glazing | SU |  | P | P |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_\_\_\_\_\_\_\_\_\_9/29/23\_\_\_\_\_\_\_\_\_\_\_\_**    **Inspector (Print Name):\_\_\_\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Nathaniel Wixon Middle School - 901 Route 134, South Dennis, Massachusetts** | | | | | |
| **Location** | **ACBM**  **Description** | **Estimated**  **Quantity** | | **VERTEX**  **April 2013**  **Condition** | **September**  **2023**  **Updated Condition** |
| ***Upper Level-Original Section (Continued)*** | | | | | |
| Room 277 Bathroom | 12" x 12" Gray Spec Floor Tile | 36 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 36 | ft2 | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Room 277 Hall | 12" x 12" Gray Spec Floor Tile | 60 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 60 | ft2 | G | G |
| Room O  (Time Out Room by 277) | 12" x 12" Gray Spec Floor Tile | 144 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 144 | ft2 | G | G |
| Room 278  (Music Room) | 12" x 12" Gray Spec Floor Tile | 1750 | ft2 | G | 2 ft2 D |
| 2' x 4' Ceiling Tile (Fissure) | 1718 | ft2 | G | 8ft2 D |
| Black Sink Mastic | 2 | Units | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 278 Bathroom | 12" x 12" Gray Spec Floor Tile | 96 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 96 | ft2 | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| 278-279 Connector Room | 12" x 12" Gray Spec Floor Tile | 240 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 240 | ft2 | G | G |
| Music Storage Room | 12" x 12" Gray Spec Floor Tile | 120 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 120 | ft2 | G | G |
| Room 279  (Music Room) | 12" x 12" Gray Spec Floor Tile | 1460 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 1460 | ft2 | G | 24ft2 D |
| Interior Window Glazing | SU |  | P | P |
| Room 217 (Art) | 12" x 12" Brown Spec Floor Tile | 1280 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 1280 | ft2 | 16 ft2 D | G |
| Black Sink Mastic | 2 |  | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 218 (Art) | 12" x 12" Brown Spec Floor Tile | 1280 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 1280 | ft2 | G | G |
| Black Sink Mastic | 2 |  | G | G |
| Interior Window Glazing | SU |  | P | P |
| Teachers Lounge | 2' x 4' Ceiling Tile (Fissure) | 960 | ft2 | 16 ft2 D | G |
| Interior Window Glazing | SU |  | P | P |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_\_\_\_\_\_\_9/29/23\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**    **Inspector (Print Name):\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Nathaniel Wixon Middle School - 901 Route 134, South Dennis, Massachusetts** | | | | | |
| **Location** | **ACBM**  **Description** | **Estimated**  **Quantity** | | **VERTEX**  **April 2013**  **Condition** | **September**  **2023**  **Updated**  **Condition** |
| ***Upper Level-Original Section (Continued)*** | | | | | |
| Teachers-Mens Room | 12" x 12" Brown Spec Floor Tile | 64 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 48 | ft2 | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Teachers-Womens Room | 12" x 12" Brown Spec Floor Tile | 56 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 48 | ft2 | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Janitor Closet by Boys and Girls Room | 12" x 12" Brown Spec Floor Tile | 48 | ft2 | 8 ft2 D | 8 ft2 D |
| 2' x 4' Ceiling Tile (Fissure) | 48 | ft2 | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Girls Room by 208 | 2' x 4' Ceiling Tile (Fissure) | 192 | ft2 | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Room 212 | 12" x 12" Gray Spec Floor Tile | 420 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 420 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 210 | 12" x 12" Gray Spec Floor Tile | 900 | ft2 | 24 ft2 D | 24 ft2 D |
| 2' x 4' Ceiling Tile (Fissure) | 900 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 209 | 12" x 12" Gray Spec Floor Tile | 900 | ft2 | G | 1 ft2 D |
| 2' x 4' Ceiling Tile (Fissure) | 900 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 206 | 12" x 12" Gray Spec Floor Tile | 900 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 900 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 205 | 12" x 12" Gray Spec Floor Tile | 900 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 900 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 204 (Science) | 12" x 12" Brown Spec Floor Tile | 1010 | ft2 | G | 10 ft2 D |
| 2' x 4' Ceiling Tile (Fissure) | 1010 | ft2 | G | 24ft2 D |
| Interior Window Glazing | SU |  | P | P |
| Fixed Laboratory Bench Tops | 150 | ft2 | G | G |
| Fire Blanket (Assumed) | 1 | Unit | G | G |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_9/29/23**    **Inspector (Print Name):\_\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Nathaniel Wixon Middle School - 901 Route 134, South Dennis, Massachusetts** | | | | | |
| **Location** | **ACBM**  **Description** | **Estimated**  **Quantity** | | **VERTEX**  **April 2013**  **Condition** | **September**  **2023**  **Updated**  **Condition** |
| ***Upper Level-Original Section (Continued)*** | | | | | |
| Room 203 (Science) | 12" x 12" Brown Spec Floor Tile | 1234 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 1208 | ft2 | 64 ft2 D | G |
| Interior Window Glazing | SU |  | P | P |
| Fixed Laboratory Bench Tops | 300 | ft2 | G | G |
| Fume Hood (Assumed) | 1 | Unit | G | G |
| Room 202/201 | 12" x 12" Brown Spec Floor Tile | 1010 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 1010 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Fire Blanket (Assumed) | 1 | Unit | G | G |
| 201-212 Corridor | 2' x 4' Ceiling Tile (Fissure) | 3204 | ft2 | 40 ft2 D | 8 ft2 D |
| Interior Window Glazing | SU |  | P | P |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Boys Locker Room | 12" x 12" Brown Spec Floor Tile | 60 | ft2 | G | G |
| 12" x 12" Gray Spec Floor Tile | 1080 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 60 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Dot)\* | 954 | ft2 | G | G |
| Drywall/Joint Compound | 270 | ft2 | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Boys Locker Room Office and Closet | 12" x 12" Gray Spec Floor Tile | 160 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 152 | ft2 | G | G |
| Boys Locker Room Office Bathroom | 12" x 12" Gray Spec Floor Tile | 42 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Dot)\* | 42 | ft2 | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Boys Locker Room Bathroom | 12" x 12" Gray Spec Floor Tile | 120 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 136 | ft2 | 8 ft2 D | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Boys Locker Room Shower Room | 2' x 4' Ceiling Tile (Dot)\* | 450 | ft2 | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Stair # 1 to Archive (Former Girls Locker Room) | 2' x 4' Ceiling Tile (Fissure) | 252 | ft2 | G | G |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_\_\_\_\_\_9/29/23\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**    **Inspector (Print Name):\_\_\_\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Nathaniel Wixon Middle School - 901 Route 134, South Dennis, Massachusetts** | | | | | |
| **Location** | **ACBM**  **Description** | **Estimated**  **Quantity** | | **VERTEX**  **April 2013**  **Condition** | **September**  **2023**  **Updated**  **Condition** |
| ***Upper Level-Original Section (Continued)*** | | | | | |
| Archive (Former Girls Locker Room) | 2' x 4' Ceiling Tile (Fissure) | 16 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Dot)\* | 1584 | ft2 | G | D 16ft2 |
| Pipe Fitting Insulation  (In Wall Chase Opening) | 21 | Units | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Archive Storage A | 12" x 12" Gray Spec Floor Tile | 140 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 140 | ft2 | G | G |
| Archive Storage B | 2' x 4' Ceiling Tile (Fissure) | 180 | ft2 | G | 2ft2D |
| Archive Storage C, Bathroom and Closet | 12" x 12" Gray Spec Floor Tile | 200 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 140 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Dot)\* | 60 | ft2 | G | G |
| Pipe Fitting Insulation (Assumed Behind Wall) |  |  | U | U |
| Archive Bathroom | 12" x 12" Gray Spec Floor Tile | 100 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 100 | ft2 | G | G |
| Pipe Fitting Insulation (Assumed Behind Wall) |  |  | U | U |
| Janitor Closet in Stair Adjacent to Archive | 12" x 12" Gray Spec Floor Tile | 36 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 36 | ft2 | G | G |
| Storage Closet in Stair Adjacent to Archive | 12" x 12" Gray Spec Floor Tile | 224 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 216 | ft2 | 8 ft2 D | 8 ft2 D |
| Stair # 2 to Archive (Former Girls Locker Room) | 2' x 4' Ceiling Tile (Fissure) | 252 | ft2 | G | G |
| Gym Storage | 12" x 12" Gray Spec Floor Tile | 384 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 384 | ft2 | 144 ft2 D | G |
| Pipe Fitting Insulation | 21 | Units | G | G |
| Gym | Flexible Duct Connector Cloth | 2 | Units | G | G |
| Auditorium | 2' x 4' Ceiling Tile (Fissure) | 5300 | ft2 | G | Abated |
| Stage Room # 2 (By Auditorium Lobby) | 12" x 12" Gray Spec Floor Tile | 1080 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 1080 | ft2 | G | G |
| Flexible Duct Connector Cloth | 2 | Units | G | G |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_\_\_\_\_\_9/29/23\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**    **Inspector (Print Name):\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Nathaniel Wixon Middle School - 901 Route 134, South Dennis, Massachusetts** | | | | | |
| **Location** | **ACBM**  **Description** | **Estimated**  **Quantity** | | **VERTEX**  **April 2013**  **Condition** | **September**  **2023**  **Updated**  **Condition** |
| ***Upper Level-Original Section (Continued)*** | | | | | |
| Stage | Wood Flooring Paper (Assumed) | 1400 | ft2 | C | C |
| 2' x 4' Ceiling Tile (Fissure) | 1400 | ft2 | G | Abated |
| Stage Curtains (Assumed) |  |  | G | G |
| Stage Room # 1 (By Main Entrance Lobby) | 12" x 12" Gray and Brown Spec Floor Tile | 750 | ft2 | G | G |
| Auditorium/Cafeteria/Gym Corridor | 2' x 4' Ceiling Tile (Fissure) | 736 | ft2 | G | G |
| Cafeteria | 12" x 12" Brown Spec Floor Tile | 3800 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Kitchen Locker Area and Bathroom | 12" x 12" Gray Spec Floor Tile | 100 | ft2 | G | G |
| 12" x 12" Brown Spec Floor Tile | 48 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 150 | ft2 | G | G |
| Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Kitchen Pantry | 2' x 4' Ceiling Tile (Fissure) | 80 | ft2 | G | G |
| Cafeteria/Gym Storage Closet | 12" x 12" Gray Spec Floor Tile | 200 | ft2 | G | 2 ft2 D |
| 2' x 4' Ceiling Tile (Fissure) | 200 | ft2 | 8 ft2 D | 8 ft2 D |
| Cafeteria/Gym Storage Closet | 2' x 4' Ceiling Tile (Fissure) | 40 | ft2 | G | 4ft2 D |
| Former Girls Room by 103 | Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Girls Locker Room | Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Girls Locker Room Storage Closet | 2' x 4' Ceiling Tile (Fissure) | 4 | ft2 | G | G |
| ***Lower Level-Original Section*** | | | | | |
| 201-101 Stair | 2' x 4' Ceiling Tile (Fissure) | 280 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 102 | 12" x 12" Brown Spec Floor Tile | 880 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 103 | 12" x 12" Brown Spec Floor Tile | 900 | ft2 | G | 2 ft2 D |
| Interior Window Glazing | SU |  | P | P |
| Room 104 | 12" x 12" Gray Spec Floor Tile | 890 | ft2 | G | 4 ft2 D |
| Interior Window Glazing | SU |  | P | P |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_9/29/23**    **Inspector (Print Name):\_\_\_\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Nathaniel Wixon Middle School - 901 Route 134, South Dennis, Massachusetts** | | | | | |
| **Location** | **ACBM**  **Description** | **Estimated**  **Quantity** | | **VERTEX**  **April 2013**  **Condition** | **September**  **2023**  **Updated**  **Condition** |
| ***Lower Level-Original Section (Continued)*** | | | | | |
| Room 105 | 12" x 12" Gray Spec Floor Tile | 900 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 106 | 12" x 12" Gray Spec Floor Tile | 900 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 107 | 12" x 12" Gray Spec Floor Tile | 900 | ft2 | G | 10 ft2 D |
| Interior Window Glazing | SU |  | P | P |
| 206-107 Stair | 2' x 4' Ceiling Tile (Fissure) | 280 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 109 | 12" x 12" Gray Spec Floor Tile | 900 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 110 | 12" x 12" Brown Spec Floor Tile | 900 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 111 | 12" x 12" Brown Spec Floor Tile | 900 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| 210-111 Stair | 2' x 4' Ceiling Tile (Fissure) | 280 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Room 113 | 12" x 12" Brown Spec Floor Tile | 224 | ft2 | G | G |
| Womens Room by 113 | 2' x 4' Ceiling Tile (Fissure) | 136 | ft2 | G | 8 ft2 D |
| Pipe Fitting Insulation (Assumed Behind Wall) |  |  | U | U |
| Mens Room by 113 | 2' x 4' Ceiling Tile (Fissure) | 8 | ft2 | G | G |
| Pipe Fitting Insulation (Assumed Behind Wall) |  |  | U | U |
| Room 115 | 12" x 12" Brown Spec Floor Tile | 1200 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 1192 | ft2 | G | G |
| Interior Window Glazing | SU |  | P | P |
| Electrical Room adjacent to Room 115 | 12" x 12" Gray Spec Floor Tile | 120 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 120 | ft2 | 16 ft2 D | G |
| Room 116/115 Connector Room | 12" x 12" Gray Spec Floor Tile | 170 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 130 | ft2 | 24 ft2 D | G |
| Room 117 | Interior Window Glazing | SU |  | P | P |
| Library Offices # 1, 2 and 3 | 12" x 12" Gray Spec Floor Tile | 544 | ft2 | G | G |

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **AHERA Six-Month Surveillance Inspection Date:\_9/29/23\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**    **Inspector (Print Name):\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_**  **Nathaniel Wixon Middle School - 901 Route 134, South Dennis, Massachusetts** | | | | | |
| **Location** | **ACBM**  **Description** | **Estimated**  **Quantity** | | **VERTEX**  **April 2013**  **Condition** | **September**  **2023**  **Updated**  **Condition** |
| ***Addition Section*** | | | | | |
| Library | 12" x 12" Gray Spec Floor Tile (Under Carpet) | 3360 | ft2 | G | G |
| Contaminated Carpet |  |  | G | G |
| Library Storage | 12" x 12" Gray Spec Floor Tile | 460 | ft2 | G | G |
| 2' x 4' Ceiling Tile (Fissure) | 460 | ft2 | U | G |
| Boys Room by Room 109 | Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | U | U |
| Girls Room by Room 107 | Pipe Fitting Insulation  (Assumed Behind Wall) |  |  | G | G |
| Storage 135 | 12" x 12" Gray Spec Floor Tile | 460 | ft2 | G | G |
| ***Addition Section*** | | | | | |
| Room 140 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 141 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 142 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 143 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 144 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 146 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 315 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 316 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 317 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 318 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 319 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 320 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 321 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Room 314 | Black Sink Mastic\*\* | 1 | Unit | G | G |
| Loading Dock | 2' x 4' Ceiling Tile (Fissure) | 16 | ft2 | G | 1ft2 |

Notes:

ft2 = Square Foot Cond. = Condition U = Unknown

lf = Linear Foot G = Good C = Covered

Unit = Each MD = Minor Damage NF = Not Found

Y= Yes D = Damaged NPI = Not Previously Identified

N = No Fri. = Friable SU = Store Front Window Units