|  |
| --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_\_3/7/22****Inspector (Print Name):\_\_\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Location: Ezra Baker Elementary School - 810 Route 28 West Dennis, Massachusetts** |
| **Location** | **ACBM****Description**  | **Estimated** **Quantity** | **VERTEX****2013****Condition** | **March****2022****Updated****Condition** |
| ***Addition Section-Upper Level*** |
| Room 118 | 9" x 9" Blue Floor Tile and Mastic (Under Carpet) | 900 | ft2 | C | Abated |
| Contaminated Carpet | 900 | ft2 | G | Abated |
| Room 138/Bathroom | Black Residual Mastic | 190 | ft2 | C | C |
| 12" x 12" Tan Streak Floor Tile (Contaminated) | 190 | ft2 | G | G |
| Room 119/Staff Lunch | Black Residual Mastic | 900 | ft2 | C | C |
| 12" x 12" Beige Spec Floor Tile (Contaminated) | 900 | ft2 | G | MD 4ft2 |
| Elevator Area/Hall | Black Residual Mastic | 260 | ft2 | C | C |
| 12" x 12" Beige Spec Floor Tile (Contaminated) | 260 | ft2 | G | 3ft2 D |
| Room 117 | 9" x 9" Gray/Tan Floor Tile and Mastic (Under Carpet) | 800 | ft2 | C | Abated |
| Contaminated Carpet | 800 | ft2 | G | Abated |
| Room 115 | 9" x 9" Gray/Tan Floor Tile and Mastic (Under Carpet) | 800 | ft2 | C | Abated |
| Contaminated Carpet | 800 | ft2 | G | Abated |
| Room 113 | 9" x 9" Gray/Tan Floor Tile and Mastic (Under Carpet) | 800 | ft2 | C | Abated |
| Contaminated Carpet | 800 | ft2 | G | Abated |
| Janitor Closet by Room 111 | Black Residual Mastic | 50 | ft2 | C | C |
| 12" x 12" Brown Streak Floor Tile (Contaminated) | 50 | ft2 | G | 2ft2D |
| Room 111 | 9" x 9" Gray/Tan Floor Tile and Mastic (Under Carpet) | 800 | ft2 | C | Abated |
| Contaminated Carpet | 800 | ft2 | G | Abated |
| Room 114 | 9" x 9" Gray/Tan Floor Tile and Mastic (Under Carpet) | 800 | ft2 | C | Abated |
| Contaminated Carpet | 800 | ft2 | G | Abated |
| Room 112 | 9" x 9" Blue Floor Tile and Mastic (Under Carpet) | 800 | ft2 | C | Abated |
| Contaminated Carpet | 800 | ft2 | G | Abated |
| Corridor # 1 (Rm 118-111) | Black Residual Mastic | 1560 | ft2 | C | Abated |
| 12" x 12" Tan Streak Floor Tile (Contaminated) | 1560 | ft2 | G | Abated |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_\_\_\_\_3/7/22\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Inspector (Print Name):\_\_\_\_\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Location: Ezra Baker Elementary School - 810 Route 28 West Dennis, Massachusetts** |
| **Location** | **ACBM****Description**  | **Estimated** **Quantity** | **VERTEX****2013****Condition** | **March****2022****Updated****Condition** |
| ***Addition Section-Upper Level (Continued)*** |
| Room 101 | 9" x 9" Gray/Tan Floor Tile and Mastic (Under Carpet) | 960 | ft2 | C | Abated |
| Contaminated Carpet | 960 | ft2 | G | Abated |
| Room 102 | 9" x 9" Gray/Tan Floor Tile and Mastic (Under Carpet) | 960 | ft2 | C | Abated |
| Contaminated Carpet | 960 | ft2 | G | Abated |
| Room 103 | 9" x 9" Gray/Tan Floor Tile and Mastic (Under Carpet) | 960 | ft2 | C | Abated |
| Contaminated Carpet | 960 | ft2 | G | Abated |
| Janitor Closet by Nurse Clinic | 9" x 9" Gray/Tan Floor Tile and Mastic  | 60 | ft2 | 4 ft2 D | Abated |
| Attic  | Flexible Duct Connector Cloth  | 2 | Units | G | G |
| Nurse Clinic | 9" x 9" Gray Floor Tile and Mastic  | 10 | ft2 | G | Abated |
| Black Residual Mastic | 600 | ft2 | C | C |
| 12" x 12" Tan Streak Floor Tile (Contaminated) | 600 | ft2 | G | G |
| Corridor # 2 (Rm 101-Nurse Clinic) | Black Residual Mastic | 860 | ft2 | C | C |
| 12" x 12" Tan Streak Floor Tile (Contaminated) | 860 | ft2 | G | Abated |
| Room 104 | 9" x 9" Dark Brown Floor Tile and Mastic (Under Carpet) | 900 | ft2 | C | Abated |
| Contaminated Carpet | 900 | ft2 | G | Abated |
| Room 105 | 9" x 9" Dark Brown Floor Tile and Mastic (Under Carpet) | 900 | ft2 | C | Abated |
| Contaminated Carpet | 900 | ft2 | G | Abated |
| Room 106/Main Office | 9" x 9" Dark Brown Floor Tile and Mastic (Under Carpet) | 900 | ft2 | C | Abated |
| Contaminated Carpet | 900 | ft2 | G | Abated |
| Principal Office  | Black Residual Mastic | 460 | ft2 | C | Abated |
| 12" x 12" Gray Spec Floor Tile (Contaminated) | 460 | ft2 | G | Abated |
| Principal Office Storage and Bathroom | 9" x 9" Dark Brown FT and Mastic  | 60 | ft2 | G | Abated |
| Pipe and Fitting Insulation (Assumed behind Wall) | U |  | U | U |

|  |
| --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_\_\_3/7/22****Inspector (Print Name):\_\_\_\_\_\_\_\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Location: Ezra Baker Elementary School - 810 Route 28 West Dennis, Massachusetts** |
| **Location** | **ACBM****Description**  | **Estimated** **Quantity** | **VERTEX****2013****Condition** | **March****2022****Updated****Condition** |
| ***Addition Section-Upper Level (Continued)*** |
| Conference Room | Black Residual Mastic | 180 | ft2 | C | Abated |
| 12" x 12" Gray Spec Floor Tile (Contaminated) | 180 | ft2 | G | Abated |
| Vice Principal Office  | Black Residual Mastic | 144 | ft2 | C | C |
| 12" x 12" Gray Spec Floor Tile (Contaminated) | 144 | ft2 | G | Abated |
| Corridor # 3 (Nurse Clinic-Vice Principal) | Black Residual Mastic | 980 | ft2 | C | Abated |
| 12" x 12" Tan Streak Floor Tile (Contaminated) | 980 | ft2 | G | Abated |
| Corridor # 4 (Main Office-Room 118) | Black Residual Mastic | 680 | ft2 | C | Abated |
| 12" x 12" Tan Streak Floor Tile (Contaminated) | 680 | ft2 | G | Abated |
| ***Original Section-First Floor*** |
| Room 107 | Wood Flooring Paper (Assumed) | 600 | ft2 | C | C |
| Pipe Insulation  | 24 | lf  | MD | MD |
| Janitor Closet by Room 107 | 9" x 9" Dark Brown Floor Tile and Mastic | 12 | ft2 | D | Abated |
| Mens Room by Main Stair  | Pipe Insulation  | 75 | lf  | G | G |
| Mens Room Chase  | Pipe Insulation  | 15 | lf  | D | D |
| Pipe Fitting Insulation  | 33 | Units | G | G |
| Bathroom Corridor/Main Stair | Black Residual Mastic | 260 | ft2 | C | Abated |
| 12" x 12" Tan Streak Floor Tile (Contaminated) | 260 | ft2 | G | Abated |
| Bathroom Corridor/Main Stair Closet | 9" x 9" Dark Brown Floor Tile and Mastic | 40 | ft2 | G | Abated |
| Womens Room by Main Stair | Pipe Insulation  | 30 | lf  | G | G |
| Pipe Fitting Insulation  | 1 | Unit | G | G |
| Pipe and Fitting Insulation (Assumed behind Wall) |  |  | U | U |
| Room 108 | Wood Flooring Paper (Assumed) | 720 | ft2 | C | Abated |
| Mens Room by 109 | Pipe Insulation  | 12 | lf  | G | G |
| Pipe and Fitting Insulation (Assumed behind Wall) |  |  | U | U |

|  |
| --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_\_\_\_\_\_3/7/22\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Inspector (Print Name):\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Location: Ezra Baker Elementary School - 810 Route 28 West Dennis, Massachusetts** |
| **Location** | **ACBM****Description**  | **Estimated** **Quantity** | **VERTEX****2013****Condition** | **March** **2022****Updated****Condition** |
| ***Original Section-First Floor (Continued)*** |
| Womens Room by 110 | Pipe Insulation  | 36 | lf  | G | G |
| Pipe and Fitting Insulation (Assumed behind Wall) |  |  | U | U |
| Room 109 | Wood Flooring Paper (Assumed) | 600 | ft2 | C | C |
| Pipe Insulation  | 12 | lf  | MD | MD |
| Room 110 | Wood Flooring Paper (Assumed) | 600 | ft2 | C | C |
| Pipe Insulation  | 45 | lf  | G | G |
| 1st Floor Corridor (107-Gym) and (Main Stair -110) | Black Residual Mastic | 1100 | ft2 | C | Abated |
| 12" x 12" Tan Streak Floor Tile (Contaminated) | 1100 | ft2 | G | Abated |
| Wood Flooring Paper (Assumed) | 1100 | ft2 | C | Abated |
| Gym/Stage  | Wood Flooring Paper (Assumed) | 6300 | ft2 | C | C |
| Gym Storage (Right of Stage) | Wood Flooring Paper (Assumed) | 260 | ft2 | C | C |
| Pipe Insulation  | 25 | lf  | 10 lf D  | Abated |
| Pipe Fitting Insulation  | 5 | Units  | G | Abated |
| Flexible Duct Connector Cloth  | 20 | ft2 | G | Abated |
| Gym Chair Storage (Left of Stage) | Wood Flooring Paper (Assumed) | 260 | ft2 | C | C |
| Pipe Insulation  | 20 | lf  | 4 lf D | Abated |
| Pipe Fitting Insulation  | 5 | Units  | 1 D  | Abated |
| Flexible Duct Connector Cloth  | 20 | ft2 | G | Abated |
| ***Original Section-Second Floor***  |
| 204/Library | Wood Flooring Paper (Assumed) | 880 | ft2 | C | C |
| 202 | Wood Flooring Paper (Assumed) | 620 | ft2 | C | C |
| 200 | Wood Flooring Paper (Assumed) | 150 | ft2 | C | C |
| 201 | Wood Flooring Paper (Assumed) | 620 | ft2 | C | C |
| 203 | Wood Flooring Paper (Assumed) | 620 | ft2 | C | Abated |
| 205 | Wood Flooring Paper (Assumed) | 620 | ft2 | C | C |
| 2nd Floor Corridor  | 12" x12” Green Spec FT and Mastic | 740 | ft2 | 4 ft2 D | Abated |
| ***Original Section-Basement***  |
| Upper Boiler Room (Electrical Room) | Pipe Insulation  | 112 | lf | G | G |
| Pipe Fitting Insulation | 24 | Units | 7 D  | 7 D |
| Lower Boiler Room | Interior Boiler Materials  | 2 | Boilers | U | U |

|  |
| --- |
| **AHERA Six-Month Surveillance Inspection Date 3/7/22\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Inspector (Print Name):\_\_\_\_\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Location: Ezra Baker Elementary School - 810 Route 28 West Dennis, Massachusetts** |
| **Location** | **ACBM****Description**  | **Estimated** **Quantity** | **VERTEX****2013****Condition** | **March****2022****Updated****Condition** |
| ***Original Section-Basement (Continued)*** |
| Room 127 | Pipe Insulation  | 30 | lf | G | G |
| Pipe Fitting Insulation | 5 | Units | G | G |
| Pipe Insulation (Above Ceiling) | 60 | lf | G | G |
| Pipe Fitting Insulation (Above Ceiling) | 25 | Units | G | G |
| Room 129 | Pipe Insulation  | 84 | lf | G | Abated |
| Pipe Fitting Insulation | 11 | Units | G | Abated |
| Janitor Closet by 128 | Pipe Insulation  | 15 | lf | D | D |
| Pipe Fitting Insulation | 1 | Unit | G | G |
| Room 128 | Pipe Insulation  | 25 | lf | G | G |
| Pipe Fitting Insulation | 4 | Units | G | G |
| Pipe Insulation (Above Ceiling) | 60 | lf | G | G |
| Pipe Fitting Insulation (Above Ceiling) | 25 | Units | G | G |
| Room 12**6** | Pipe Insulation (Above Ceiling) | 209 | lf | G | 1 D |
| Pipe Fitting Insulation (Above Ceiling) | 23 | Units | G | G |
| Boys Room by Stair  | Pipe Insulation  | 2 | lf  | D  | Abated |
| Pipe Insulation (Above Ceiling) | 26 | lf | G | Abated |
| Pipe Fitting Insulation (Above Ceiling) | 1 | Unit | G | Abated |
| Girls Room by Stair  | Pipe Insulation  | 28 | lf  | 3 lf D  | Abated |
| Pipe Fitting Insulation | 18 | Units | G | Abated |
| Stair by Girls Room | Pipe Insulation  | 15 | lf  | G | Abated |
| Pipe Fitting Insulation | 6 | Units | G | Abated |
| Front Stair to Back Stair Corridor | Pipe Insulation  | 40 | lf | G | Abated |
| Pipe Fitting Insulation | 6 | Units | G | Abated |
| Room 126 to Side (Gym) Stair Corridor | Pipe Insulation  | 122 | lf | G | Abated |
| Pipe Fitting Insulation | 22 | Units | G | Abated |
| Boys Locker Room  | Pipe Insulation  | 85 | lf | 2 lf D  | Abated |
| Pipe Fitting Insulation  | 11 | Units | G | Abated |
| Pipe and Pipe Fitting Insulation (Assumed behind Wall) | Unknown  |  | U | Abated |

|  |
| --- |
| **AHERA Six-Month Surveillance Inspection Date:\_\_\_\_\_\_\_\_\_\_3/7/22\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Inspector (Print Name):\_\_\_\_\_\_\_\_\_\_\_\_Russell Mealey\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Inspector Signature:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_****Location: Ezra Baker Elementary School - 810 Route 28 West Dennis, Massachusetts** |
| **Location** | **ACBM****Description**  | **Estimated** **Quantity** | **VERTEX****2013****Condition** | **March****2022****Updated****Condition** |
| ***Addition Section-Lower Level*** |
| Room 141 | Pipe Insulation  | 36 | lf | G | Abated |
|  | Pipe Fitting Insulation | 4 | Units | G | Abated |
| Room 143 (E) | Pipe Insulation  | 30 | lf | G | Abated |
|  | Pipe Fitting Insulation | 10 | Units | G | Abated |
| Room 144 (F) | Pipe Insulation  | 15 | lf | G | Abated |
|  | Pipe Fitting Insulation | 5 | Units | G | Abated |
| Music Room | Pipe Insulation  | 30 | lf | G | Abated |
|  | Pipe Fitting Insulation | 2 | Units | G | Abated |
| Art Room  | Pipe Insulation  | 20 | lf | G | Abated |
| Room 139 | Pipe Insulation  | 50 | lf | G | Abated |
| Kitchen Storage  | Interior Window Glazing (Assumed) | 1 | Unit | G | G |
| Interior Window Caulking (Assumed) | 1 | Unit | G | G |
| Custodial Mop Sink Area by Kitchen | 9" x 9" Gray/Tan/Blue Floor Tile and Mastic  | 225 | ft2 | 4 ft2 D | Abated |
| Rear Delivery Entrance  | 9" x 9" Brown Floor Tile and Mastic  | 50 | ft2 | G | Abated |
| Room 132 | Pipe Insulation Debris (Above Ceiling at Entrance) | 2 | lf | Debris | Abated |
| Room 131 | Pipe Fitting Insulation (Above Ceiling) | 10 | Units | G | G |
| Room 130-131 Hallway | Pipe Fitting Insulation (Above Ceiling) | 6 | Units | G | G |

Notes:

ft2 = Square Foot Cond. = Condition U = Unknown

lf = Linear Foot G = Good C = Covered

Unit = Each MD = Minor Damage NF = Not Found

Y= Yes D = Damaged NPI = Not Previously Identified

N = No Fri. = Friable

**Notes/Updated Changes:**